CHAN. USE DIM/Addr CHAN. USE DIM/Addr

| 1 | DSR Area 1 (Door) | 24 |  | 60 | HL LED Mover Side Truss | 2/320 |
| --- | --- | --- | --- | --- | --- | --- |
| 2 | DSR Area 2 | 31 |  | 61 | HR FOH 1 LED Mover Wash | 2/340 |
| 3 | DSCR Area 3 | 34 |  | 62 | HC FOH 1 LED Mover Wash | 2/360 |
| 4 | DSCL Area 4 | 40 |  | 63 | HL FOH 1 LED Mover Wash | 2/380 |
| 5 | DSL Area 5 | 46 |  | 64 | HR LED Mover Side Truss | 2/300 |
| 6 | DSL Area 6 (Door) | 53 |  |  |  |  |
| 7 | MSR Area 7 | 79 |  | 65 | HL LED Rogue Spot | 2/400 |
| 8 | MSCR Area 8 | 80 |  | 66 | HR LED Rogue Spot | 2/425 |
| 9 | MSCL Area 9 | 81 |  |  |  |  |
| 10 | MSL Area 10 | 78 |  | 67 | HL IQ | P1. 32 P2. 2/1 |
| 11 | USR Area 11 | 66 |  | 68 | HC IQ | P1. 39 P2. 2/5 |
| 12 | USCR Area 12 | 67 |  | 69 | HR IQ | P1. 45 P2. 2/9 |
| 13 | USCL Area 13 | 68 |  |  |  |  |
| 14 | USL Area 14 | 69 |  | 70 | SR LED CYC | 2/450 |
|  |  |  |  | 71 | CS LED CYC | 2/460 |
| 20 | DSR LED Top | 2/200 |  | 72 | SL LED CYC | 2/470 |
| 21 | DSC LED Top | 2/205 |  | 75 | Mirror Ball | 4 ND |
| 22 | DSL LED Top | 2/210 |  | 80 | Chauvet LED Slimpar | 2/100 |
| 23 | MSR LED Top | 2/215 |  | 81 | Chauvet LED Slimpar | 2/110 |
| 24 | MSC LED Top | 2/220 |  | 82 | Chauvet LED Slimpar | 2/120 |
| 25 | MSL LED Top | 2/225 |  | 83 | Chauvet LED Slimpar | 2/130 |
| 26 | USR LED Top | 2/230 |  | 84 | Chauvet LED Slimpar | 2/140 |
| 27 | USC LED Top | 2/235 |  | 85 | Chauvet LED Slimpar | 2/150 |
| 28 | USL LED Top | 2/240 |  |  |  |  |
| 29 | Podium Top | 72 |  |  |  |  |
|  |  |  |  | 101 | HL Cat Special | 27 |
| 30 | DSR LED Gobo Tip | 2/250 |  | 102 | HCL Cat Special | 36 |
| 31 | DSL LED Gobo Tip | 2/255 |  | 103 | HCR Cat Special | 41 |
| 32 | MSR LED Gobo Tip | 2/260 |  | 104 | HR Cat Special | 51 |
| 33 | MSL LED Gobo Tip | 2/265 |  |  |  |  |
| 34 | USL LED Gobo Tip | 2/270 |  |  |  |  |
| 35 | USL LED Gobo Tip | 2/275 |  | 110 | LX1 SR Special 1 | 93 |
|  |  |  |  | 111 | LX1 C Top Special 2 | 94 |
| 36 | MSR Tip | 87 |  | 112 | LX1 SL Special 2 | 95 |
| 37 | MSL Tip | 84 |  | 113 | LX2 SR Special 1 | 110 |
| 38 | USR Tip | 105 |  | 114 | LX2 SL Special 2 | 114 |
| 39 | USR Tip | 119 |  |  |  |  |
| 40 | SL LED Side | 2/480 |  | 150 | House Lights | 17,23,37,187,188,189,55 |
| 41 | SR LED Side | 2/485 |  | 151 | Work Lights | 140 |
|  |  |  |  | 152 | HR Map | 55 |
| 43 | HL Top Torm grn | 19 |  | 195 | DMX Dowser | 2/475 |
| 44 | HL Mid Torm red | 20 |  | 205 | Wireless DMX | 8 ND (**P**) |
| 45 | HL Bot Torm blu | 21 |  | 210 | IQ Power Supply | 7 ND (**P**) |
| 46 | HR Top Torm grn | 59 |  | 249 | Hazer Power Supply | 9 ND |
| 47 | HR Mid Torm red | 58 |  | 250 | Radiance Hazer | 2/500 |
| 48 | HR Bot Torm blu | 57 |  |  |  |  |
| 49 |  |  |  |  |  |  |
| 50 |  |  |  |  |  |  |
| 51 |  |  |  | 500 | Lobby LED’s | 2/450 |
|  |  |  |  | 501 | Lobby LED’s | 2/460 |
| Hot Pwr. | Hot power Circuits | 11,18,25,70,74,89, |  | 502 |  |  |
|  |  | 98,107,117,123 |  | 503 |  |  |